Wastewater Treatment Plant Flow Calculations for Facilities in Broward County

Based on the most recent 12-month rolling Annual Average Daily Flow Data

(April 2016 – March - 2017)

| **PLANT NAME** | **LICENSED CAPACITY** | **COMMITTED FLOWS PER BLDG. PERMITS****AS OF****MARCH 31st 2017** | **ANNUAL AVERAGE DAILY FLOW** | **TOTAL FLOW** | **TOTAL FLOW % OF LICENSED CAPACITY** |
| --- | --- | --- | --- | --- | --- |
|  | (MGD-AADF) | (MGD) | (MGD) | (MGD) | (%) |
| BCN | BC North Reg. | 95.00 | 2.450 | 64.04 | 66.49 | 69.99% |
| COO | Cooper City | 3.44 | 0.078 | 2.52 | 2.60 | 75.58% |
| CSI | Coral Springs | 7.72 | 0.054 | 4.09 | 4.14 | 53.63% |
| DA2 | Davie 2 | 4.85 | 0.114 | 2.12 | 2.23 | 45.98% |
| DRF | Davie MBR | 3.50 | 0.000 | 1.12 | 1.12 | 32.00% |
| FER | Ferncrest | 0.545 | 0.008 | 0.29 | 0.300 | 55.05% |
| GTL | G.T. Lohmeyer | 48.00 | 1.340 | 38.23 | 39.57 | 82.44% |
| HOL | Hollywood | 55.50 | 1.640 | 34.58 | 36.22 | 65.26% |
| I-75 | I-75 Rest stop | 0.025 | 0.000 | 0.008 | 0.008 | 32.00% |
| MAR | Margate | 8.78 | 0.197 | 6.18 | 6.38 | 72.67% |
| MIR | Miramar | 12.70 | 0.419 | 9.48 | 9.90 | 77.95% |
| PPI | Pembroke Pines | 9.50 | 0.358 | 6.15 | 6.51 | 68.53% |
| PLA | Plantation | 17.50 | 0.263 | 11.82 | 12.08 | 69.03% |
| POM | Pompano Reuse | 7.50 | 0.000 | 2.43 | 2.43 | 32.40% |
| SSA | Sunrise Sawgrass | 20.00 | 0.442 | 12.40 | 12.84 | 64.20% |
| SSP | Sunrise Springtree | 10.00 | 0.041 | 7.64 | 7.68 | 76.80% |
| SSW | Sunrise Southwest | 0.45 | 0.002 | 0.34 | 0.342 | 76.00% |
|  | Total | 305.01 | 7.41 | 203.42 | 210.82 | 69.12% |

**This Report is for general information purposes only. For specific capacity analyses, or Large User Allocations, contact the Treatment Plant directly**.